Install:

Unzip ftann.zip in Matlab Work directory.



How to use:

Run ftann.m (type ftann in Matlab Command Window)
(WARNING!) Tested under Matlab R14 v7.0 


1.) Please use right mouse button to select at least 4 points on image.
    Points on image  must correspond to points on 2D model shown in Info panel.
    You can also Load/Save points from/to Matlab .mat file. Sample file Image_1.mat 
    corresponds to Image_1.jpg and Image_2.mat corresponds to Image_2.jpg. 
    
    Notice: If you select only 4 points on image, 3 of them must not be collinear.

	   	
2.) Click on 'Compute DLT' to compute homography.


3.) In Show panel, select one of the options and then left click on image in 
    Preview panel.




Authors: Ljubisa Crnadak, Nenad Burgic
	 Faculty of Electrical Engineering, Banja Luka
	 Republic of Srpska, Bosnia and Herzegovina